	
TABLE 1

MINIMUM REQUIREMENTS FOR ALL ZONING DISTRICTS


	DISTRICT

	MINIMUM
LOT AREA
IN SQ. FT.
	LOT SIZE

WIDTH
	MAXIMUM PERCENT
OF LOT TO BE 
OCCUPIED
	MAXIMUM HEIGHT 
OF BUIDINGS
      IN                  IN
  STORIES       FEET
	MINUMUM FEET REQUIREMENTS

	
	
	
	
	
	
FRONT
	
SIDE
	
REAR

	R-100
	12,000
	100’
	30
	2.5
	35
	30
	15
	25

	R-80
	7,000
	70’
	35
	2.5
	35
	25
	10
	20

	R-70
	8,000
	60’
	40
	4.0
	45
	20
	10
	20

	M-11

	3,600
	36’
	--
	2.0
	20
	20
	15
	12

	B-1
	N/R*
	N/R*
	30
	3.0
	35
	30
	+
	25

	B-2
	X
	X
	X
	N/R*
	N/R*
	N/R*
	N/R*
	20

	B-3
	N/R*
	N/R*
	60
	4.0
	45
	30
	25
	25

	

	
	
	
	
	
	
	
	

	M-1
	N/R*
	N/R*
	N/R*
	4.0
	50
	50
	25
	50

	M-2
	43,560*
	N/R*
	50
	4.0
	50
	100
	50
	50

	
	
	
	
	
	
	
	
	



*NR – No Restrictions

X –  It is the intent of this Ordinance that lots of sufficient size used for any business or service must provide sufficient standing, 
      unloading, and loading space in addition to the space required for other normal operations of the use conducted on the lot.

*  -  Not specified, except on a lot adjoining a residential lot (See specific zone for requirements).

*  -  Buildings may cover up to 100 percent of the remaining lot area after all requirements specified by this Ordinance have
        been met.  

